Toyota Tundra CHMSL 
Harness Installation

1. Disconnect and isolate the negative battery cable.
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2. Remove the Front Door Scuff Plate and the Cowl Side Trim.
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3. Remove the Intrument Panel Under Cover.
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4. Locate the OEM Stop Lamp Switch and disconnect the connector (red).
5. Plug one side of the 007-234 T-Harness into the OEM connector and the other side into the OEM Stop Lamp Switch.
6. Route the rest of the harness through a drain plug in the floor, to the back of the vehicle, and plug it into the aftermarket 3rd brake light.
7. Follow steps 1-4 in reverse order to reinstall the removed trim panels and reconnect vehicle battery.
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